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Basic Scaffold Check for Workers

	Site Address
	


	Date 
	


	Full Name of worker conducting the check
	

	Signature

	



	
	Yes
	No

	Is there an Unsafe Tag or Safe Tag by the entry point?

	
	

	Has the scaffold been inspected within the last 7 days (after any alteration or adverse weather event)? 
	
	

	Does the ladder extend 1m past the entry point?

	
	

	Is there a self-closing gate by the entry point?

	
	

	Is the scaffold fully decked out?

	
	

	Are there toeboards installed all around to prevent objects from falling?
	
	

	Is there a Top and Mid Rail?

	
	

	Is there an internal handrail for any scaffold more than 300mm away from the work surface? 
	
	

	Is there a need to secure the ladder from unauthorised entry while the scaffold is not in use? 
	
	




Remember NOT to alter scaffolding! If it is not suitable for the task – get in touch with the scaffolder and have them alter the scaffold. 



